Media Server 25.2
Media Server Help

# GUID

The Milestone GUID of the camera that the events should be associated with (the GUID of the camera that supplied the video). For information about finding the camera GUID, refer to the Milestone documentation.

You do not have to specify the camera GUID if you are ingesting video using the Milestone ingest engine. If you do not specify a GUID, Media Server automatically associates alarms to the camera that the Milestone ingest engine received the video from.

Type: | String
Default: |
Required: | Yes, unless you are ingesting video from Milestone using the Milestone ingest engine
Configuration Section: | TaskName
Example: |
See Also: |

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.2

Topic Title: GUID