View Component 25.2
View Component Help

# [IDOLServerN] Section

Use this section when you are using a unified configuration with the Distributed Action Handler and Distributed Index Handler components for a distributed setup. In this case, you configure DAH and DIH in the unified configuration file, and distribute actions to child Content components.

Each `[IDOLServerN]` section define the host and port of a child Content component that the DAH and DIH communicate with.

Use this section to define the child server configurations when you use `[DistributionIDOLServers]` and use the same child severs for DAH and DIH.

You must number child server sections in consecutive order, starting from 0 (zero).

For example:

    [DistributionIDOLServers]
    Number=2

    [IDOLServer0]
    Host=localhost
    Port=9010

    [IDOLServer1]
    Host=1.23.45.6
    Port=9010

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery View Component 25.2

Topic Title: [IDOLServerN] Section