Media Server 25.3
Media Server Help

# MaxRemoteAnalysisConnections

The maximum number of requests, for remote analysis, to accept from other Media Servers simultaneously. This number includes requests that are being processed (the number of which is limited by RemoteAnalysisConfigurations) and the number that are queued.

A remote analysis task waits for a record to be processed and returned before sending another, so this is equivalent to the maximum number of remote analysis tasks that you should configure to send records to this Media Server.

Each connection requires an ACI thread, so ensure that you set the value of Threads to be greater than the value of this parameter.

Type: | Integer
Default: | 10
Required: | No
Configuration Section: | Chaining
Example: | `MaxRemoteAnalysisConnections=6`
See Also: | RemoteAnalysisConfigurations

Copyright 2025 Open Text
Version 25.3 | Last updated July 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.3

Topic Title: MaxRemoteAnalysisConnections