Media Server 25.3
Media Server Help

# MaxInputQueueLength

Analysis tasks usually do not process every frame of a video. An analysis task chooses frames to process at regular intervals throughout the video. This interval is called the sample interval. Analysis engines have a default sample interval, and if the engine supports the `SampleInterval` configuration parameter you can choose a sample interval.

When Media Server encounters a complex section of video with lots of activity in the scene, the time required to process each video frame can increase. When the time required is longer than the sample interval, subsequent frames have to wait before Media Server is ready to process them. This is normal and ensures that the frames selected for analysis are evenly distributed.

This parameter specifies the maximum delay that is acceptable between a video frame being ingested and it being analyzed. For example, if you set `MaxInputQueueLength=3s` then Media Server discards any video frame that has been waiting longer than three seconds (effectively increasing the sample interval).

Setting this parameter therefore places a limit on latency, which is the amount of time between a video frame being ingested by Media Server and data being output. The total latency is the value of this parameter plus the time required to analyze the frame. In some cases, such as a number plate recognition system installed in a police car, it is extremely important to have low latency. However, in complex sections of video with lots of activity, Media Server might be forced to discard video frames that could otherwise have been processed.

IMPORTANT: Setting this parameter can reduce accuracy and reduce the number of events that are identified.

OpenText recommends that you explore alternatives before setting this parameter. For example, if the analysis engine supports using multiple threads and your Media Server has sufficient resources, you could increase the number of CPU threads used for analysis, so that Media Server can process several video frames concurrently. To increase the number of threads, use the configuration parameter `NumParallel`.

IMPORTANT: Do not set this parameter unless you have set the parameter IngestRate to `1`.

Type: | Time duration The value of this parameter is a time duration. Specify a value using one or more of the following units:
         days          d
         hours         h
         minutes       m
         seconds       s
         milliseconds  ms
         microseconds  us
For example, all of the following are equivalent:
         1minute 3seconds
         1m 3s
         63s
To specify an infinite duration, use the value `Infinite`.
Default: | (No limit)
Required: | No
Configuration Section: | TaskName
Example: | `MaxInputQueueLength=5s`
See Also: |

Copyright 2025 Open Text
Version 25.3 | Last updated July 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.3

Topic Title: MaxInputQueueLength