Media Server 25.3
Media Server Help

# Configure the Downstream Media Server

This section describes how to configure Media Server to receive records from another Media Server and continue processing them.

To receive records from another Media Server

1. Create a new configuration file, or open an existing configuration that you want to modify.

2. In the `[Session]` section, add a new task by setting the `EngineN` parameter. You can give the task any name, for example:

       [Session]
       Engine0=RecordsFromUpstream

3. Create a new configuration section by typing the task name inside square brackets. Then, set the following parameters:

   `Type` | The ingest engine to use. Set this parameter to `Receive`.
   `Input` | A comma-separated list of tracks to receive from the other Media Server.

   For example:

       [RecordsFromUpstream]
       Type=Receive
       Input=FaceDetect.ResultWithSource
       // or using alias "DetectedFaces", if defined in upstream configuration:
       // Input=DetectedFaces

4. Configure the analysis, encoding, ESP, and output tasks that you want to run on the ingested records.

   NOTE: The tracks produced by the `Receive` engine are prefixed with the name of the ingest task. For example, if you use the configuration above the track produced by the `Receive` engine is named:

   - `RecordsFromUpstream.FaceDetect.ResultWithSource` (if no alias is defined).
   - `RecordsFromUpstream.DetectedFaces` (if the alias `DetectedFaces` is defined by the upstream Media Server).

   You must use the correct track name for the input of your face recognition task on the downstream Media Server.

5. Save the configuration file in the location specified by the `ConfigDirectory` parameter.

Copyright 2025 Open Text
Version 25.3 | Last updated July 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.3

Topic Title: Configure the Downstream Media Server