Media Server 25.3
Media Server Help

# Location

A comma-separated list of ISO-3166 codes to specify the locations for which you want to recognize number plates. Specify the primary location first.

For example, if you are recognizing number plates in France but also want to recognize plates from Germany and Belgium, set this parameter to `Location=FR,DE,BE`. The first location is assigned the priority `1.0`, and subsequent locations are assigned the priority `0.01` (indicating those plates are 100 times less likely to be seen). If you want to set the relative priority for each location, set the parameter LocationWithPriorities instead.

There are significant differences in the number plates used by countries and states, so to read the plates successfully you must set either this parameter or LocationWithPriorities.

To obtain a list of supported locations with ISO-3166 codes, use the action ListNumberPlateLocations.

If you want to read plates for a location that is not supported, you can set `Location=NOF` (to recognize plates without matching detected characters to number plate formats).

Type: | String
Default: |
Required: | Yes, unless you set LocationWithPriorities
Configuration Section: | TaskName
Example: | `Location=FR,DE,BE`
See Also: | LocationWithPriorities

Copyright 2025 Open Text
Version 25.3 | Last updated July 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.3

Topic Title: Location