Media Server 25.3
Media Server Help

# Example Configuration

The following is an example configuration that runs news segmentation on ingested video. This configuration runs segmentation using a Content component that is on the same machine as Media Server. It also includes an output task to write the results of segmentation to files on disk.

    [Ingest]
    IngestEngine=AV

    [AV]
    Type=Video

    [Analysis]
    AnalysisEngine0=SpeechToText
    AnalysisEngine1=TextSegmentation
    AnalysisEngine2=NewsSegmentation

    [SpeechToText]
    Type=SpeechToText
    Language=ENUS
    Mode=relative
    ModeValue=0.90
    FilterMusic=true

    [TextSegmentation]
    Type=TextSegmentation
    Input=SpeechToText.Result

    [NewsSegmentation]
    Type=NewsSegmentation
    Input=TextSegmentation.Result
    IdolHost=localhost
    IdolPort=9000

    [Output]
    OutputEngine0=XML

    [XML]
    Type=xml
    Input=NewsSegmentation.Result,SpeechToText.Result
    Mode=bounded
    EventTrack=NewsSegmentation.Result
    XMLOutputPath=./output/%token%/Story_%segment.type%_%segment.sequence%.html

Copyright 2025 Open Text
Version 25.3 | Last updated July 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.3

Topic Title: Example Configuration