Distributed Action Handler 26.1
Distributed Action Handler Help

# Configure SSL in a Unified System

Use the following procedure to configure SSL in a setup where you configure the DAH in the unified configuration file.

To configure an SSL connection in a unified system

1. Open the unified configuration file in a text editor.

2. Find the `[Server]` section, the `[IDOLServerN]` or `[DAHEngineN]` section, or a combination of the `[Server]` section and one of the others.

3. Add the SSLConfig setting to specify the section in which you have set the SSL details for the connection, usually `SSLOptionN`. For example:

       [Server]
       (other server settings...)
       SSLConfig=SSLOption0

       [IDOLServer0]
       SSLConfig=SSLOption0

       [IDOLServer1]
       SSLConfig=SSLOption1

   In this example, incoming ACI calls and outgoing calls to `IDOLServer0` share the same SSL configuration, and outgoing calls to `IDOLServer1` use a different configuration.

4. Create an `[SSLOptionN]` section for each unique SSLConfig setting. Each `SSLOption` entry must contain the SSLMethod, SSLCertificate, and SSLPrivateKey parameters. For example:

       [SSLOption0]
       SSLMethod=TLSV1.3
       SSLCertificate=host1.crt
       SSLPrivateKey=host1.key

       [SSLOption1]
       SSLMethod=TLSV1.3
       SSLCertificate=host2.crt
       SSLPrivateKey=host2.key

5. Save and close the configuration file. Restart the unified Knowledge Discovery service for your changes to take effect.

Copyright 2025 Open Text
Version 26.1 | Last updated January 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Distributed Action Handler 26.1

Topic Title: Configure SSL in a Unified System