Media Server 26.1
Media Server Help

# RTSPTransport

The transport protocol to use when the source is an RTSP stream. You can use any value supported by the FFmpeg option `rtsp_transport`.

Type: | String
Default: |
Required: | No
Configuration Section: | TaskName
Example: | `RTSPTransport=udp`
See Also: |

Copyright 2025 Open Text
Version 26.1 | Last updated January 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 26.1

Topic Title: RTSPTransport