Octane Connector 26.1
Octane Connector Help

# ThreadStatus

Displays a list of all ACI threads and specifies what each thread is doing.

## Example

    http://12.3.4.56:9000/action=ThreadStatus

This action uses port `9000` to request thread information from a component, which is located on a machine with the IP address `12.3.4.56`.

## Optional Parameters

This action accepts the following standard ACI action parameters.

Parameter | Description
--- | ---
ActionID | A string to use to identify an ACI action.
FileName | The file to write output to.
ForceTemplateRefresh | Forces the server to load the template from disk.
Output | Writes output to a file.
ResponseFormat | The format of the action output.
Template | The template to use for the action output.
TemplateParamCSVs | A list of variables to use for the specified template.

Copyright 2025 Open Text
Version 26.1 | Last updated January 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Octane Connector 26.1

Topic Title: ThreadStatus