Media Server 26.2
Media Server Help

# Use Multiple Media Servers

It is possible to configure multiple Media Servers to use the same rolling buffer configuration file. You can have a maximum of one Media Server writing video into a rolling buffer, but other Media Servers can read content from the rolling buffer.

If you configure multiple Media Servers to use the same rolling buffer configuration file, you must:

- grant read access to the rolling buffer configuration file to all of the Media Servers.
- grant write access to the rolling buffer configuration file to only one Media Server. If you need to change the settings for your rolling buffers, you must send actions to this Media Server.
- allow only one Media Server to write video into each rolling buffer. The `Stream` parameter in a rolling buffer encoding task specifies which rolling buffer to write video to.

Copyright 2026 Open Text
Version 26.2 | Last updated April 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 26.2

Topic Title: Use Multiple Media Servers