Media Server 26.2
Media Server Help

# Receive Ingest Engine

The Receive ingest engine ingests information (images or video frames, and metadata) that was output by another Media Server. For information about how to split processing across multiple Media Servers, see Chain Media Servers.

To configure a task that uses the Receive ingest engine, you can set the following parameters:

Configuration Parameter | Description
--- | ---
Input | A comma-separated list of tracks to receive from the other Media Server.
Type | The type of ingest engine to use. Set this parameter to `Receive`.

The engine produces a track for each track specified by the `Input` parameter. For example, if you set `Input=FaceDetect.ResultWithSource`, the engine produces a track named `taskName.FaceDetect.ResultWithSource`, where `taskName` is the name of the Receive ingest task.

Copyright 2026 Open Text
Version 26.2 | Last updated April 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 26.2

Topic Title: Receive Ingest Engine