Quest Archive Manager Connector 26.2
Quest Archive Manager Connector Help

# TCPReceiveWindowSize

The TCP receive window size to use when the service receives data (in bytes).

Use this parameter to tune network performance based on bandwidth and client to server round-trip times. Generally, a higher value improves performance in a high-bandwidth, high-delay network, and a lower value improves performance in a low-bandwidth, low-delay network.

Type: | Long
Default: | Determined by the operating system
Allowed Range: | Minimum: 1024 Maximum: 1048576
Required: | No
Configuration Section: | Service
Example: | `TCPReceiveWindowSize=65536`
See Also: |

Copyright 2026 Open Text
Version 26.2 | Last updated April 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Quest Archive Manager Connector 26.2

Topic Title: TCPReceiveWindowSize