FileNet P8 Connector 26.3
FileNet P8 Connector Help

# Service Configuration Parameters

The parameters in this section configure the service port, which provides service status information.

You must enable the service port by specifying the ServicePort configuration parameter, and you must configure authorization roles to determine which users can send service requests (see Authorization Roles Configuration Parameters). The service port then accepts the standard status and control actions described in Service Actions.

Parameter | Description
--- | ---
Access-Control-Allow-Origin | A list of URLs that you want to use to access the Knowledge Discovery Admin interface.
FIPSMode | Enables FIPS-compliant cryptographic modules.
LogGSSFailures | Enables logging for GSS authentication failures.
RequireGSSAuth | Enables GSSAPI authentication mode on the service port.
ServiceHost | The host server on which the service is running.
ServicePort | The port to listen on, for service status and control requests.
SSLConfig | The name of a section in the configuration file that contains the service port SSL configuration.
TCPReceiveWindowSize | The TCP receive window size to use when the service receives data (in bytes).
XSLTemplates | Enables the transformation of service action responses using XSL templates.

Copyright 2026 Open Text
Version 26.3 | Last updated July 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery FileNet P8 Connector 26.3

Topic Title: Service Configuration Parameters