GuideWire Connector 26.3
GuideWire Connector Help

# DataPort

The `DataPort` parameter specifies the port used as the data port for the ACI server. This port is used for transferring files to and from the connector.

Type: | Long
Default: |
Required: | No
Allowed Range: | Minimum: 1 Maximum: 65535
Configuration Section: | Server
Example: | `DataPort=7011`
See Also: |

Copyright 2026 Open Text
Version 26.3 | Last updated July 2026

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery GuideWire Connector 26.3

Topic Title: DataPort