Open topic with navigation

# Pushing a Subscriber Configuration

A pushed subscriber configuration synchronizes the configuration from ArcMC to all or a selection of the configuration’s subscribers. Pushing must be performed manually.

When selecting subscribers, only valid potential subscribers for the configuration are shown. For example, if pushing a Logger configuration, which only applies to Loggers, only managed Loggers would be shown as potential subscribers, not Connector Appliances or ArcMCs.

Note: If a configuration push to the localhost fails, restart the web service on the localhost.

To push a subscriber configuration to all subscribers:

1. Select Configuration Management > All Subscriber Configurations.

   Tip: To filter for a specific subscriber configuration type, select the desired configuration type from the Subscriber Configurations sub-menu.

2. From the Configurations table, select a configuration to be pushed.

3. Click Push.

4. Click Yes to confirm the push. The configuration is pushed to all subscribers of the selected configuration. A compliance check is automatically performed on each subscriber.

To push a subscriber configuration to selected subscribers:

1. Select Configuration Management > Subscriber Configurations > All Configurations.

   Tip: To filter for a specific subscriber configuration type, select the desired configuration type from the Subscriber Configurations sub-menu.

2. From the Configurations table, select a configuration to be pushed, and click the name of the configuration.

3. On the Configuration Details and Subscribers page, click the Subscribers tab.

4. On the Subscribers tab, select one or more subscribers to which to push the configuration.
5. Click Push.

6. Click Yes to confirm the push. The configuration is pushed to the selected subscribers. A compliance check is automatically performed on each recipient.