Content Manager 24.4 Content Manager

# On-line scanners

Your on-line scanner does not need to have an in-built clock, as each scan will update the Content Manager dataset immediately.

All it needs to do is read Code 39 barcodes and send them to the computer in ASCII format through a serial cable.

NOTE: For scanners that use the USB port, refer to the manufacturer's documentation for installing drivers that mimic a serial port.

Copyright 2008-2024 Open Text
Version 24.4 | Last updated October 2024
Contact

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to hprmdocumentation@microfocus.com.

We appreciate your feedback!

Product: Content Manager 24.4

Topic Title: On-line scanners