Open topic with navigation

# VideoProfile

The profile to use for encoding video. The profile specifies the video codec, video bitrate, and so on.

Set this parameter to one of the following values:

- `mpeg4video_h264_hd`
- `mpeg4video_h264_720p`
- `mpeg4video_h264_360p`
- `mpeg4video_h264_sd`
- `mpeg2video`
- `mpeg2video_broadcast`

The MPEG4 profiles use the H264 codec for encoding video and are suitable for playback over the web, for example if your users view video using the HPE MMAP Media Player or the native player of a web browser that supports H264. HPE recommends using the MPEG4 profiles in most cases, but you can use the MPEG2 profiles if you need to support a media player that cannot decode H264.

For more information about these profiles, refer to the HPE Media Server Administration Guide.

Type: | String
Default: | mpeg2Video
Required: | No
Configuration Section: | TaskName
Example: | `VideoProfile=mpeg4video_h264_hd`
See Also: | AudioProfile

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm