Open topic with navigation

# MJPEG_HTTP Ingest

The MJPEG_HTTP ingest engine ingests MJPEG video that is streamed over HTTP.

Configuration Parameter | Description
--- | ---
StreamTimeout | The maximum number of seconds to wait for the next frame.
Type | The type of ingest engine to use. Set this parameter to `MJPEG_HTTP`.

The MJPEG_HTTP engine produces the following tracks:

- an image track, named `Image_1`.
- a proxy track, named `taskName.Proxy`, where `taskName` is the name of the ingest task.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm