Open topic with navigation

# Memory Requirements

The amount of memory required by HPE Media Server depends on many factors, including the type of tasks that you run. The following table provides minimum memory requirements for some analysis tasks.

The requirements listed below are the same regardless of the number of media sources that you process concurrently, and the number of threads that are used for each task.

Analysis Task | Memory Requirement
--- | ---
Face analysis
Face detection | 25 MB
Face recognition | 65 MB
Face demographics | 42 MB
Vehicle analysis
Vehicle make recognition | 43 MB
Image classification
Image classification | 55 MB
Additional memory required for the pre-trained ImageNet classifier | 240 MB
Additional memory required for the pre-trained road scene classifier | 50 MB
Object detection
Object detection | 18 MB
Additional memory required for the pre-trained person detector | 340 MB
Additional memory required for the pre-trained road scene detector | 338 MB
Optical Character Recognition
OCR | 28 MB
Additional memory required for Simplified Chinese text | 40 MB
Additional memory required for Traditional Chinese text | 53 MB
Additional memory required for Japanese text | 31 MB
Additional memory required for Korean text | 13 MB

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm