Open topic with navigation

# SpeedBiasLevel

The balance between speed and accuracy in the decoder.

By default, `SpeedBiasLevel` is set to `0`, which leaves the underlying parameter settings untouched (that is, quick configuration of relevant parameters is disabled).

To enable the speed configuration, set `SpeedBiasLevel` to a value between `1` (slowest) and `6` (fastest). The default speech-to-text parameters are equivalent to a speed bias of `2`.

NOTE:

You can use the `SpeedBiasLevel` functionality only when the speech-to-text mode is `fixed`, and with a DNN-based language resource.

Action: | AddTask
Task: | ClusterSpeechToTextTel SpeechToText SpeechToTextFilter SpeechToTextTelephony StreamToText StreamToTextMusicFilter TelWavToText WavToText
Type: | Integer
Default: | 0
Range: | 0–6
Example: | `SpeedBiasLevel=3`
See Also: | SpeedBiasLevel (configuration parameter)

© 2015-2018 EntIT Software LLC, a Micro Focus company | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm