Open topic with navigation

# Stream Live Video

To stream live video from VMS, use the following URL:

    rtsp://host:port/Accs=Live/livetrack=input/

where:

`host` | is the host name or IP address of the machine hosting VMS.
`port` | is the RTSP port, as defined by the Port parameter in the `[RTSP]` section of the configuration file. You can also find the RTSP port by using the action GetRtspPort.
`input` | is the index number for the video input (camera).

For example, to view live video from the fourth camera, use the following URL:

    rtsp://vms:554/Accs=Live/livetrack=3/

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm