Open topic with navigation

# GetRtspSessions

The `GetRtspSessions` action returns a summary of the RTSP clients that are taking video from VMS.

Active sessions are sessions that are currently receiving video from VMS. Init sessions are sessions that have finished.

Ready sessions are sessions that are no longer active but for which an RTSP TEARDOWN method has not been received. Ready sessions should time-out and be moved to Init sessions. If there is no RTSP activity, there should be no Ready sessions. If there are, this might indicate a problem with VMS's RTSP server.

The number of Active sessions added to the number of Init sessions gives the maximum number of concurrent sessions reached since VMS started.

## Example

    http://localhost:15000/action=GetRtspSessions

## Response

    <summary>3 Active Sessions, 10 Init sessions, 0 Ready sessions</summary>
    <session>Client 1 active@ 10.2.110.107</session>
    <session>Client 2 active@ 10.2.110.107</session>
    <session>Client 3 active@ 10.2.110.107</session>

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm