# Crop Transformation Engine

The crop transformation engine produces cropped images. The region data is usually supplied by an analysis task. For example, after running face detection you can use this engine to produce cropped images that show detected faces. Alternatively, you can crop images to a fixed region by setting the `Region` parameter, in which case region data in the input records are ignored.

The engine also translates any co-ordinates contained in records, so that their position is correct for the cropped image. For example, face detection outputs the locations of a person's eyes. The co-ordinates are modified so that the positions are correct for the cropped image.

Configuration Parameter | Description
--- | ---
Border | The amount of padding to add to the supplied region, before cropping the image.
BorderUnit | The units to use for specifying the value of the Border configuration parameter.
Input | The name of the track that contains the images to crop, with region data.
Region | Specifies the region to use when cropping the image. Set this parameter only when you want to specify a fixed region.
RegionUnit | The units to use to specify the position and size of the region.
Type | The type of transformation engine to use. Set this parameter to `crop`.

This transformation engine produces a single output track, named `taskName.Output`, where `taskName` is the name of the transformation task.

© Copyright 2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm