Media Server 25.1
Media Server Help

# Source

The media source to process. Specify one of the following:

- a path to a file residing on a file system that Media Server can access. To strengthen security, Media Server can be configured to read files only from specified directories. For information about the directories that Media Server is permitted to read from, see the parameter AllowedInputDirectories.
- the URL of a stream.
- the name of a DirectShow device (to ingest from a DirectShow source, such as a capture card).

- to ingest video using the Milestone ingest engine, specify either:

  - a camera name (not supported with XProtect Corporate when you set MilestoneDirectory).
  - a camera UUID.

  - (Milestone XProtect Corporate only) a camera UUID followed by a stream ID, in the following format:

        id:camera_uuid,streamid:stream_id

    If your camera produces multiple streams and you do not specify a stream ID, Media Server ingests the stream that is configured as the default in the Milestone XProtect system.

- to ingest video using the Genetec Ingest Engine, specify a camera logical ID.

Actions: | Process
Type: | String
Default: |
Example: | The following example specifies the path to a file: `Source=./videoarchive/broadcast.mpeg` The following example specifies a camera ID and stream ID, for ingesting from a Milestone XProtect Corporate system: `Source=id:939690e7-634c-4f70-844e-b6a079db0177,streamid:2762d39d-a779-4ac8-bdb7-91aab494ebe8`
See Also: |

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.1

Topic Title: Source