Media Server 25.3
Media Server Help

# Audio Categorization Results

The following XML shows a single record produced by audio categorization.

    <record>
      <timestamp>
        <startTime iso8601="1970-01-01T00:00:01Z">1000000</startTime>
        <duration iso8601="PT00H00M00.500000S">500000</duration>
        <peakTime iso8601="1970-01-01T00:00:01Z">1000000</peakTime>
        <endTime iso8601="1970-01-01T00:00:01.500000Z">1500000</endTime>
      </timestamp>
      <trackname>AudioCategorize.Result</trackname>
      <AudioCategorizeResult>
        <id>e8d84838-bdf2-4b9b-9a92-e7e42b249103</id>
        <category>Music</category>
        <confidence>80</confidence>
      </AudioCategorizeResult>
    </record>

The record contains the following information:

- The `id` element contains the identifier for the audio segment.

- The `category` element shows how the audio segment was classified. The categories are pre-defined and this value can be:

  - `DialTone`
  - `DTMF-*`, `DTMF-0`, `DTMF-1`, `DTMF-2`, and so on. These values indicate that the audio contains a DTMF tone. For example, `DTMF-2` indicates the tone for the "2" button.
  - `Music`
  - `Noise`
  - `Silence`
  - `Speech`

  NOTE: Dial tone and DTMF tone detection are enabled only when you process audio with a sample rate of 8KHz.

- The `confidence` element provides the confidence score for the classification, from 0 to 100, where 100 indicates the greatest confidence.

Copyright 2025 Open Text
Version 25.3 | Last updated July 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.3

Topic Title: Audio Categorization Results